Electrical Lighting Controls Schedule

Revision Date Description Created Checked

T1 2 Tender Issue

**Schedule of Equipment – Single floor hard wired**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Code** | **Description** | **iLight Series** | **Product Code** | **Image** | **Areas** |
| LCM1 | 2 Universe DALI Controller  (128 addresses) | iLight  Enterprise | SCMD2 | **Graphical user interface  Description automatically generated** | Open plan office/meeting room |
| LCM2 | 4 Universe DALI Controller  (256 addresses) | iLight  Enterprise | SCMD4 | Graphical user interface  Description automatically generated | Open plan office/meeting room |
| P1 | Miniature DALI PIR/Photocell, 32mm cut out, for integration into a luminaire | iLight Enterprise | PPAD- C-MB-DALI ADDR | A close-up of a computer mouse  Description automatically generated with medium confidence | Recess, Luminaire or Besa integrated |
| P2 | HB DALI Ceiling mount PIR/photocell, 64mm cut out | iLight Enterprise | PPAD-C-HB-DALI-ADDR | **A picture containing light  Description automatically generated** | High Bay - Atriums & Warehouses |
| FD1 | DALI field relay  On of/off control | iLight Enterprise | FLTS | Text  Description automatically generated | For control of non-dimmable luminaires via DALI |
| CP1 | Plastic DALI Control Plate White | iLight Enterprise | CLD Range | Graphical user interface, diagram  Description automatically generated | Meeting rooms |
| CP2 | Plastic DALI Control Plate Black | iLight Enterprise | CLD Range |  | Meeting rooms |
| UI-1 | DALI Input Unit | iLight Enterprise | DALI-I-U | A picture containing text, cable, thread, connector  Description automatically generated | Switch input module via DALI |
| TS1 | 8” Multiroom Colour Touchscreen | iLight Enterprise | TSE80 | A picture containing text, monitor, black, indoor  Description automatically generated | Reception, meeting rooms or central controller |
| TS2 | 5.5” Multiroom Colour Touchscreen | iLight Enterprise | TSE55 | A picture containing text, monitor, screenshot  Description automatically generated | Reception, meeting rooms or central controller |
| UI-2 | Mini Universal Interface  For Room Partition | iLight Enterprise | UIM | Diagram  Description automatically generated | Connection of switch contacts to CAN and room partition switches |